**MULTI-POINT VEHICLE INSPECTION**

(Check body condition)

(Check lamps)

**ONSTAR DIAGNOSTICS**

OnStar Active

Enrolled in Advanced Diagnostics Report Dealer Maintenance Notification

Service History/Recall Check

**ENGINE OIL AND FILTER**

Engine oil

Oil Life Monitor %

Reset Oil Life Monitor

**LIGHTS**

Exterior lights

**WINDSHIELD AND WIPERS**

Wiper blade—driver Wiper blade—passenger Wiper blade—rear Windshield condition Cracks

Chips

**BATTERY**

Battery condition\*

See attached battery printout Battery cables and connections

Battery voltage

**VEHICLE AND FUNCTIONAL INSPECTIONS**

**Inspect (Fit, Form, and Function)**

Safety belt components

**Check Operation**

Horn Ignition lock

Starter switch

Evaporative control system

**VISIBLE LEAK INSPECTION**

Engine oil Transmission

Engine cooling system Power steering

Brake fluid reservoir Windshield washer fluid Transfer case

Fuel system Drive axle

Diesel exhaust fluid

Accelerator pedal

Passenger-compartment air filter Floor mat fit and wear Compartment lift struts

Engine air filter Hoses

Belts

Shocks and struts Steering components

Axle boots or driveshaft and U-joints

Exhaust system

**Filled**

**Lubricate**

Chassis components

**ADDITIONAL NOTES**

Technician:

Advisor:

\*Courtesy battery testing can provide early warning of a potential battery failure. More extensive testing and analysis may be necessary to verify the actual need for battery replacement and/or warranty reimbursement. ©2017 General Motors. All rights reserved. All text, images, and other content in this document are subject to the copyright and other intellectual property rights of GM. These materials may not be reproduced, distributed, or modified without the express written permission of GM.

CS-MPVI-GENERIC-17

Checked and OK

May require attention soon Requires immediate attention Not inspected if not indicated

**BRAKES** Front Brakes: Good: 7 mm or greater Rear Brakes: Good: 4 mm or greater OK: 6 mm to 4 mm OK: 3 mm

Bad: 3 mm or less Bad: 2 mm or less

**Front Brakes Rear Brakes**

Driver front: /mm Driver rear: /mm

Passenger front: /mm Passenger rear: /mm

Brake system Parking Brake

**TIRE INSPECTION**

**Driver Side Front Passenger Side Front**

PSI before: PSI set to: PSI before: PSI set to: Tread depth: /32 Tread depth: /32

Wear pattern/damage Wear pattern/damage

**Driver Side Rear Passenger Side Rear**

PSI before: PSI set to: PSI before: PSI set to: Tread depth: /32 Tread depth: /32

Wear pattern/damage Wear pattern/damage

Rotation needed Reset tire pressure monitor

Alignment needed Tire sealant expiration date:

Balance needed

**Year/Make/Model: Repair Order #:**

**VIN:**

**Name:**

**Date: Recommended Next Service:**