VEHICLE INSPECTION

INSPECTION POINT

INSPECTION POINT

PASS FAIL

PASS

FAIL

1

Foot brakes (pads/shoes thickness)

9

Turn indicator lights

Min. per manufacturer:

Front Rear

Stop Lights

10

Front Brake Left

Measurements

11

Front seat adjustment

Front Brake Right

Measurements

12

Doors (open, close, lock)

Rear Brake Left

Measurements

13

Horn

Rear Brake Right

Measurements

14

Speedometer

Emergency brake (parking

brake)

2

Bumpers

15

3

Steering mechanism

16

Muffler and exhaust system

Ball joints

17

Tires, incl. tread depth

Tie rods

Right front

[32nd’s / In]

Rack & pinion

Left front

[32nd’s / In]

Bushings

Right rear

[32nd’s / In]

4

Windshield

Left rear

[32nd’s / In]

Large crack

Interior and exterior rear view mirrors

18

Small crack

19

Safety belts for driver and passenger(s)

5

Rear window and other glass

6

Windshield wipers

7

Headlights

Tail lights

8

RASIER PARTNER NAME

EMAIL ADDRESS

RASIER PARTNER SIGNATURE

RASIER PARTNER PHONE NUMBER

DATE

**TO BE COMPLETED BY INSPECTOR**

COMPANY

VEHICLE MILEAGE

LICENSE PLATE #

VIN#

VEHICLE MAKE

VEHICLE MODEL

VEHICLE YEAR

ADDRESS

INSPECTOR NAME

INSPECTOR SIGNATURE

DATE

VEHICLE INSPECTION PASS FAIL

(Please circle)