***POV INSPECTION CHECKLIST***

**ITEM WHAT TO CHECK**

**LOOK FOR KNOWN DEFICIENCIES**

**CHECK OFF**

**TIRES**

Condition

***NOTE: No mixing of radial tires and bias tires.***

Spare tire

Tread depth, wear, weathering, evenly seated, bulges, imbedded objects, cuts, breaks. At least one mm of tread over entire traction surface.

*(Using a penny, place it in the tire tread with head facing downward. If the tread does not reach the top of Lincoln's head, there is insufficient tread depth)*

Spare tire (inflated), jack, lug wrench

Front Rear

Pass Fail

**LIGHTS**

Head lights Tail Lights Brake lights Turn Signals Backup lights

Four-way Flashers

License Plate Light

Both high and low beams operational, cracked, condensation, secured

Lenses intact, tail light working when turned on (red)

Lenses intact, brake light working when brake is applied (red)

Lenses intact, left and right turn signals blink (red lights in rear and yellow lights in front)

Lenses intact, left and right backup lights work (White Light)

Lenses intact, left and right turn signals flash/blink at the same time

Lenses intact, does light stay on

Left Right

Left Right

Left Right

Front Rear

Left Right

Left Right

Front Rear

Left Right

Pass Fail

**WINDSHIELD & WINDOWS & WIPERS**

Windshield Rear Window Windows

Window controls Windshield wipers

Not cracked, broken or scratched to the degree that impairs vision

Not cracked, broken or scratched to the degree that impairs vision

Windows go up and down, scratched or tinted to the degree that impairs vision

Check handles, push electric buttons

Both wipers are installed on vehicle, windshield wipers work, blades show signs of wear

Pass Fail

Pass Fail

Pass Fail

Front Rear

Pass Fail

**MIRROR**

Mirror Outside

Mirror Inside

Missing, cracked, adjustable Missing, cracked, adjustable

Left Right

Pass Fail

**BUMPERS**

Bumper Front Bumper Rear

Missing, loose, broken

Missing, loose, broken, bent in any way to cause a hazard

Pass Fail

Pass Fail

**BRAKES**

Brakes Emergency Brake

Foot pedal cannot travel more than half way to floor, does brake light stay on

Properly adjusted, check emergency brake by: pull/push emergency brake, apply foot to brake, gently press gas pedal, ensure brake holds vehicle

Pass Fail

Pass Fail

**Interior**

Horn

Defroster Front

Does it work

Ensure hot air blows out above the dash

Pass Fail

Pass Fail

Inspector's

Name: Signature

Operator

Name: Signature

Platoon Sergeant/Platoon Leaders

approval

Date inspection was conducted

Date follow-up inspection was conducted Leave/Pass/Holiday

Defroster Rear

Emergency equipment

Heater

**SEATBELTS**

Seatbelt Front/Rear (Include shoulder harness during inspection, may have a center seat belt)

Check light on dash, if in the winter ensure it works by allowing the rear windshield to clear up

(OPTIONAL) First aid kit, warning triangle, flashlight, fire extinguisher, blanket, flares, shovel, chains, tools, etc.

Ensure heater works

Missing, frayed, does not snap

Pass Fail

Pass Fail

Pass Fail

Front Rear

**LICENSE/DECALS/INSURANCE**

State Drivers License

License Plate/ Inspection Decal

Insurance

Expired, missing

Expired, check sticker/decal to ensure plate is current

Does the operator have valid insurance

Pass Fail

Pass Fail

Pass Fail

**UNDER THE HOOD FLUIDS**

Brake

Windshield washer Oil

Power Steering

**HOSES**

**BATTERY**

Filled to appropriate level Windshield washer fluid Filled to appropriate level Filled to appropriate level

Cuts, cracks, leaks, bulges, chaffing, deterioration

Terminals, clean and tight, held down securely

Pass Fail

Pass Fail

Pass Fail

Pass Fail

Pass Fail

Pass Fail